***************************************************************************************************************
* This file defines optional GTN750 toolbar panel events mapping
* This is an example and you should customize and rename it to "toolbar_panel_events.txt.
* The file must be named "toolbar_panel_events.txt" and must be put into the Config/pms50-gtn750 package folder
* BE CAREFUL to save the file somewhere outside the package when you update the GTN750 version.
***************************************************************************************************************

******************
* Config section *
******************
* pollingMode can be permanent or timed
* In permanent mode the instrument reads the defined variables at each frame and permanently.
* This may impact performance if you have many variables defined here.
* In timed mode, the instrument still reads the defined variables at each frame but stops reading after
* the given time out (set in the pollingTimeOut parameter) if none of the variables has been set for the duration of the time out.
* To activate the polling in timed mode, you must set the L:GTN750_PANEL_CUSTOM_START_POLLING variable to 1.
* Typically you could set this variable before each setting of one or a group of panel variables.
* pollingTimeOut unit is millisecond. Minimum value is 10ms.
******************************************************************************************************************************************
[Config]
pollingMode=permanent
pollingTimeOut=2000


**************************
* PanelVariables section *
**************************
* This section defines all the custom variables
* Each entry has the following form:
*
* VariableName,VariableValue=EventName
*
* Where:
*
* VariableName is your custom variable name. It must contain only uppercase alphabetic and numeric characters and the underscore.
*               It must starts with the string "L:GTN750_PANEL_CUSTOM_".
* VariableValue is the variable value. It must be an integer equal or greater than 1. This is an optional field with a default value of 1.
*               Using different values for the same variable name saves FPS because we have only one variable to check.
*               However there is a risk to skip some values if you send them too quickly.
* EventName is one of the event names defined in the document events.pdf found in the "documentation" package folder
*               or online at https://pms50.com/fs2020/gtn750/events.pdf.
*               Don't use the Bezel event names as a custom event because they have their own variable names (see the manual).
******************************************************************************************************************************************
[PanelVariables]
L:GTN750_PANEL_CUSTOM_ZOOM,1=ZOOM_IN
L:GTN750_PANEL_CUSTOM_ZOOM,2=ZOOM_OUT
L:GTN750_PANEL_CUSTOM_BACK=BACK
L:GTN750_PANEL_CUSTOM_MSG=MSG
L:GTN750_PANEL_CUSTOM_MENU,1=GoToPage-HOME-MENU_HOME
L:GTN750_PANEL_CUSTOM_MENU,2=GoToPage-WEATHER-MENU_WEATHER
L:GTN750_PANEL_CUSTOM_MENU,3=GoToPage-NEAREST-MENU_NEAREST
L:GTN750_PANEL_CUSTOM_MENU,4=GoToPage-WAYPOINT_INFO-MENU_WAYPOINT_INFO
L:GTN750_PANEL_CUSTOM_MENU,5=GoToPage-SERVICES-MENU_SERVICES
L:GTN750_PANEL_CUSTOM_MENU,6=GoToPage-UTILITIES-MENU_UTILITIES
L:GTN750_PANEL_CUSTOM_MENU,7=GoToPage-SYSTEM-MENU_SYSTEM
L:GTN750_PANEL_CUSTOM_MENU,8=GoToPage-SETUP-MENU_SETUP
